{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["LV = [(1.463 x 10^7 x R^2) / (Fs^2 x Vb)] - 1.463 x R",{"$nulls":4},"Формула"]
[]
["R",0,"вътрешния радиус на тръбата в инчове"]
["Fs",null,"желаната настройка на честотата на кутията в херцове  (Hz)"]
["Vb",0,"вътрешния обем на кутията в кубически инча"]
[]
["Резултат"]
["LV",{"$error":"#DIV/0!"},"дължината на рефлектора в инчове"]
[null,{"$error":"#DIV/0!"},"дължината на рефлектора в сантиметри"]
["* 1инч = 2,54см"]
[]
["Диаметър на тръбата",null,null,null,"Обем на кутията"]
[null,"=",0,null,null,"=",0,"=",0]
["сантиметра",null,"инча",null,"литра",null,"куб.фута",null,"куб.инча"]
[{"$nulls":6},"или"]
[null,"=",0,null,null,"=",0]
["инча",null,"сантиметра",null,"куб.фута",null,"куб. Инча"]
[]
[]
[]
["Попълнете оградените в червено параметри, и ще получите необходимата дължина на фазоинвертора в синьо"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}