{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":19,"rows_kept":34,"cut":false,"hidden":false,"merged":[[13,12,13,13],[24,4,24,5],[24,6,24,7],[24,8,24,9],[24,10,24,11],[24,12,24,13],[13,4,13,5],[13,6,13,7],[13,8,13,9],[13,10,13,11],[2,12,2,13],[2,4,2,5],[2,6,2,7],[2,8,2,9],[2,10,2,11]],"flags":["formulas_cached_only"]}
[null,"Alfa  Romeo Camshaft Data :- Model 1600cc/2000cc Twin Cam ",{"$nulls":12},"NEWMAN CAMS 10",null,null,1]
[null,"Rocker Ratio 1 : 1"]
[null,"Part No","Application","Power ","Duration",null,"Valve Lift",null,"Cam Lift",null,"Timing",null,"Full Lift",null,"Valve","Clear","Price ","Material"]
[null,null,null,"Band","In","Ex","In","Ex","In","Ex","In Open","Ex Close","IN. ATDC","EX BTDC","In","Ex","Ex VAT","Type"]
[null,"ALFT/280/425","Touring/ Fast Road Cam",1500,280,280,0.425,0.423,0.425,0.423,"30-70","70-30",110,110,0.008,0.01,350,"Billet"]
[null,"PH2",null,6000,null,null,10.786802030456853,10.736040609137056,10.786802030456853,10.736040609137056,{"$nulls":4},0.2032,0.254,"Per Pair"]
[null,"Notes.","Excellent Mid Range Power ,No loss of Low Down Power, Smooth Idle"]
[null,"ALFT/300/460","Rally/ Race Cam ",3000,300,300,0.46,0.458,0.46,0.458,"42-78","82-38",112,108,0.008,0.01,350,"Billet"]
[null,"PH4",null,7500,null,null,11.6751269035533,11.624365482233504,11.6751269035533,11.624365482233504,{"$nulls":4},0.2032,0.254,"Per Pair",null," "]
[null,"Notes.","Race /Tarmac Rally Cam  only suitable for the 2 Litre  Engine  Best suited to Run with 45 or 48 DCOE Carbs "]
[{"$nulls":8}," "]
[null,"Alfa  Romeo Camshaft Data :- Model Alfa Sud/33 8 Valve Flat 4"]
[null,"Rocker Ratio 1 : 1"]
[null,"Part No","Application","Power ","Duration",null,"Valve Lift",null,"Cam Lift",null,"Timing",null,"Full Lift",null,"Valve","Clear","Price ","Material"]
[null,null,null,"Band","In","Ex","In","Ex","In","Ex","In Open","Ex Close","IN. ATDC","EX BTDC","In","Ex","Ex VAT","Type"]
[null,"ALFS/280/380","Touring/Fast Road Cam",3000,280,280,0.38,0.378,0.38,0.378,"32-69","69-31",109,109,0.008,0.01,120,"Repro"]
[null,"PH2",null,7000,null,null,9.644670050761421,9.593908629441625,9.644670050761421,9.593908629441625,{"$nulls":4},0.2032,0.254,480,"Billet"]
[null,"Notes.","Excellent Low Down Power and Smooth Tickover.On Repro Cams Machine Head/ Carrier to Retain Original Shims Size"]
[null,"ALFS/300/422","Race/ Tarmac Rally Cam",4000,300,300,0.422,0.42,0.422,0.42,"42-78","82-38",112,108,0.012,0.012,480,"Billet"]
[null,"PH4",null,8000,null,null,10.710659898477157,10.65989847715736,10.710659898477157,10.65989847715736,{"$nulls":4},0.3048,0.3048,"Per Pair"]
[null,"Notes.","Race /Tarmac Rally Cam. Other Race Profiles Available on request  "]
[]
[null,"Alfa  Romeo Camshaft Data :- Model GT V6 24 Valve"]
[null,"Rocker Ratio 1 : 1"]
[null,"Part No","Application","Power ","Duration",null,"Valve Lift",null,"Cam Lift",null,"Timing",null,"Full Lift",null,"Valve","Clear","Price ","Material"]
[null,null,null,"Band","In","Ex","In","Ex","In","Ex"," In Open","EX  Close","IN. ATDC","EX BTDC","In","Ex","Ex VAT","Type"]
[null,"ALF6/260/392","Touring / Fast Road Cam",2000,260,260,0.392,0.37,0.392,0.37,"20-60","60-20",110,110,0.012,0.012,600,"Billet"]
[null,"PH2",null,6500,null,null,9.949238578680204,9.390862944162437,9.949238578680204,9.390862944162437,{"$nulls":4},0.3048,0.3048,"Per Pair"]
[null,"Notes.","Excellent Low Down  yet free Revving  Good Tick Over"]
[null,"ALF6/300/452","Race/ Tarmac Rally. Cam",3750,300,300,0.452,0.432,0.452,0.432,"42-78","82-38",112,108,0.012,0.012,600,"Billet"]
[null,"PH4",null,8000,null,null,11.472081218274113,10.964467005076143,11.472081218274113,10.964467005076143,{"$nulls":4},0.3048,0.3048,"Per Pair"]
[null,"Notes.","Race/Tarmac Rally Good Free  Revving Cams  Giving Main power from 4500 RPM"]
[]
[null,"Audi","All Models See Volkswagon Section  Pages 36 to 39"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}