{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Time","Vehicle speed","Engine speed","Intake air quantity","Air quantity signal","TAG"]
[13.45,37.27,1479,635.1,3.001]
[14.01,37.91,1496,644.7,3.03]
[14.57,38.21,1516,650.4,2.977]
[15.13,38.82,1541,660.7,3.03]
[15.69,38.74,1535,657.6,3.04]
[16.25,38.84,1538,657.5,3.006]
[16.81,39,1546,663.5,3.006]
[17.37,39.2,1554,662.7,3.099]
[17.93,39.97,1613,835.8,3.382]
[18.49,42.25,1713,1006.5,3.71]
[19.05,45.3,1844,1321.1,4.081]
[19.61,49.68,2009,1572.8,4.296]
[20.17,54.32,2184,1703.4,4.423]
[20.73,58.71,2387,1540.1,4.326]
[21.29,63.45,2569,1381,4.33]
[21.85,67.4,2710,1353.9,4.399]
[22.41,71.2,2875,1365.4,4.453]
[22.97,75.31,3028,1331.2,4.467]
[23.53,78.77,3167,1303.1,4.516]
[24.1,82.39,3306,1298.9,4.555]
[24.66,85.73,3441,1300.8,4.599]
[25.22,89.01,3572,1282.9,4.629]
[25.78,92.31,3689,1274.9,4.658]
[26.34,95.09,3807,1264.6,4.677]
[26.9,98.14,3917,1245.8,4.697]
[27.46,100.82,4024,1245.3,4.717]
[28.02,103.29,4126,1245.3,4.741]
[28.58,105.96,4220,1245.3,4.746]
[29.14,108.09,4304,1245.3,4.751]
[29.7,110.5,4400,1245.3,4.741]
[30.26,112.66,4488,1245.3,4.741]
[30.82,114.76,4566,1245.3,4.707]